# Supported Intel® PRO/1000 Server Adapters

This driver software is designed to operate with the following Intel PRO/1000 Server Adapters:

Product Name | Distinguishing Features | LEDs | Order Code† | Board ID #†† | Controller
--- | --- | --- | --- | --- | ---
Intel® PRO/1000 Gigabit Server Adapter | SC Fiber connector, Full Duplex | 4 | PWLA8490 | 700262-xxx 717037-xxx | 82542
Intel® PRO/1000 F Server Adapter | SC Fiber connector, Full Duplex | 4 | PWLA8490SX | 738640-xxx A38888-xxx | 82543
Intel® PRO/1000 T Server Adapter | Copper RJ45 connector, supports 10/100/1000 | 3 | PWLA8490T | A19845-xxx A33948-xxx | 82543
Intel® PRO/1000 XT Server Adapter | Copper RJ45 connector, supports 10/100/1000 | 2 | PWLA8490XT PWLA8490XTLP | A51580-xxx | 82544EI
Intel® PRO/1000 XF Server Adapter | SC Fiber connector, Full Duplex | 3 | PWLA8490XF | A50484-xxx | 82544EI
Intel® PRO/1000 MT Server | Copper RJ45 connector, supports 10/100/1000 | 2 | PWLA8490MT | A92165-xxx | 82545EM
Intel® PRO/1000 MT Dual Port Server | Copper RJ45 connectors, supports 10/100/1000 | 2 | PWLA8492MT | A92111-xxx | 82545EB
Intel® PRO/1000 MF Server | LC Fiber connector, Full Duplex | 2 | PWLA8490MF | A91622-xxx | 82546EM
Intel® PRO/1000 MF Server (LX) | LC Fiber connector, 1310nm laser designed for long-haul single-mode fiber, Full Duplex | 2 | PWLA8490LX | A91624-xxx | 82546EM
Intel® PRO/1000 MF Dual Port Server | LC Fiber connectors, Full Duplex | 2 | PWLA8492MF | A91620-xxx | 82546EM

†Order Code = Printed on product packaging.
††Board ID # = A 6-digit code with a 3-digit extension; printed on barcode sticker on the front of the card.

For detailed information on these Intel adapters, see the Adapter & Driver ID Guide: http://support.intel.com/support/network

### Compatibility Notes

Intel's first generation PRO/1000 Gigabit Server Adapter has the following limitations:

- VLANs on this adapter are supported only in Microsoft Windows (Me, NT 4.0, 2000, XP and Windows Server 2003).

- Jumbo Frames on this adapter are not supported under Linux or Solaris.

- This adapter operates correctly in 32- and 64-bit slots. However, when inserted in a 64-bit PCI slot, it will incorrectly indicate that it is in a 32-bit slot.

- This adapter does not support packet tagging for QoS or VLANs.

`Last modified on 1/23/03 8:38a Revision 11`