# Attaching the Low Profile Bracket (Optional)

To install the adapter in a low profile slot, replace the standard bracket as described here.

1. Ground yourself to dissipate any static charge.

2. Remove the two screws securing the standard bracket to the back side of the adapter.

1. Slide the bracket away from the adapter.

1. Slide the low profile bracket onto the adapter.

1. Attach the low profile bracket to the adapter using the screws you removed in step 2.

1. Carefully tighten the screws until they are seated and then add 1/8 turn more. Do not over tighten.

2. Install the adapter as described above.

`Last modified on 7/23/02 10:30a Revision 4`