# Regulatory Compliance Statements

## Safety Compliance

- UL 60950 Third Edition- CAN/CSA-C22.2 No.60950-00 (USA/Canada)

- EN 60 950 (European Union)

- IEC 60 950 (International)

## EMC Compliance

- FCC Part 15 – Radiated & Conducted Emissions (USA)

- ICES-003 – Radiated & Conducted Emissions (Canada)

- CISPR 22 – Radiated & Conducted Emissions (International)

- EN55022-1998 – Radiated & Conducted Emissions (European Union)

- EN55024 - 1998 – (Immunity) (European Union)

- CE – EMC Directive (89/336/EEC) (European Union)

- VCCI – Radiated & Conducted Emissions (Japan)

- CNS13438 – Radiated & Conducted Emissions (Taiwan)

- AS/NZS3548 – Radiated & Conducted Emissions (Australia/New Zealand)

- MIC notice 1997-41, EMI and MIC notice 1997-42 – EMS (Korea)

## Regulatory Compliance Markings

When required these products are provided with the following Product Certification Markings:

- UL Recognition Mark for USA and Canada

- CE Mark

- FCC markings

- VCCI marking

- Australian C-Tick Mark

- Korea MIC mark

- Taiwan BSMI mark

## Class B Products

### FCC Class B User Information

This equipment has been tested and found to comply with the limits for a Class B digital device pursuant to Part 15 of the FCC rules. These limits are designed to provide reasonable protection against harmful interference in a residential installation. This equipment generates, uses and can radiate radio frequency energy and, if not installed and used in accordance with the instructions, may cause harmful interference to radio communications. However, there is no guarantee that interference will not occur in a particular installation.

If this equipment does cause harmful interference to radio or television reception, which can be determined by turning the equipment off and on, the user is encouraged to try to correct the interference by one or more of the following measures:

- Reorient or relocate the receiving antenna.

- Increase the separation between the equipment and receiver.

- Connect the equipment into an outlet on a circuit different from that to which the receiver is connected.

- Consult the dealer or an experienced radio/TV technician for help.

| CAUTION: If the device is changed or modified without permission from Intel, the user may void his or her authority to operate the equipment.

| NOTE: This device complies with Part 15 of the FCC Rules. Operation is subject to the following two conditions: (1) this device may not cause harmful interference, and (2) this device must accept any interference received, including interference that may cause undesired operation.

### Copper Products

- Intel® PRO/1000 XT Server Adapter

- Intel® PRO/1000 T Server Adapter

- Intel® PRO/1000 MT Desktop Adapter

## Electromagnetic Compatibility Notices

### FCC Declaration of Conformity Statement

The PRO/1000 XT Server Adapter, PRO/1000 MT Desktop Adapter, and PRO/1000 T Server Adapter have been tested to Comply with FCC Standards for Home or Office Use.

Intel Corporation
5200 N.E. Elam Young Parkway
Hillsboro, OR 97124-6497
Phone 1-800-628-8686

### Fiber Products

(Verified for FCC Class B)

- Intel PRO/1000 F Server Adapter

- Intel PRO/1000 XF Server Adapter

## Canadian Compliance (Industry Canada)

CANADA ICES-003 CLASS B / CANADA NMB-003 CLASSE B

## VCCI Class B Statement (Japan)

## MIC Notice Class B (Republic of Korea Only)

## Manufacturer Declaration
European Community

## Manufacturer Declaration

This certifies that the Intel PRO/1000 family of Gigabit Server Adapters complies with the EU Directive 89/336/EEC, using the EMC standards EN55022 and EN55024. This product also meets or exceeds EN 60950 requirements. These products have been tested and verified to meet CISPR 22 requirements.

Intel Corporation, Mailstop JF3-446
5200 N.E. Elam Young Parkway
Hillsboro, OR 97124-6497

# Class 1 Laser Product

The PRO/1000 F and PRO/1000 XF Server Adapters contain laser devices for communication use. These devices are compliant with the requirements for Class 1 Laser Products and are safe in the intended use. In normal operation the output of these laser devices does not exceed the exposure limit of the eye and cannot cause harm.

For continued safe operation in case of an abnormal circumstance, always have the provided laser connector cover in place or a compatible fiber optics cable properly connected when power is available to the product.

The Laser device must be factory serviced ONLY by the responsible manufacturer! NO adjustments, service or maintenance is to be performed otherwise.

## These Class 1 Laser devices are:

Certified and Registered with FDA/CDRH per CFR21, subchapter J.

Certified as compliant to IEC 825-1(1993) with Amendment 1(1997)and EN 60825-1 with Amendment 11(1996).

``

`Last modified on 1/14/03 2:48p Revision 5`