# PCI Hot Plug Support for NetWare* 4.11 through 6

Intel network adapters are enabled for use in selected servers equipped with PCI Hot Plug support and running NetWare* 4.11 through 6.

| NOTES: If you replace an adapter in a Hot Plug slot, do not place the removed adapter back into the same network until the server has rebooted. The two adapters may have the same virtual MAC address and create a conflict.
| PCI Hot Plug only works between identical Intel network adapters.
| Hot swapping is supported but not hot adding.

For more information on setting up and using Hot Plug support in your server, see your server's documentation.

## Using Hot Plug

Make sure you have the latest NetWare support pack installed before using Hot Plug. If your server uses any teaming features (with ANS), the driver will be loaded persistently. If teaming options are not used, the driver will unload when the slot power is off and reload when the slot is powered again. The keyword, PERSIST, can be used to control this behavior as follows:

0 = Never persist
1 = Always persist
2 = Auto persist (default). Base driver remains loaded only if ANS loaded.

| NOTE: If you are not using teaming (ANS) or VLANs, use option 1 – always persist.

`Last modified on 12/27/02 8:57a Revision 7`