			       Broadcom Corporation
			      16215 Alton Parkway,
			     Irvine, CA 92619-7013

				  Release Notes 
				Broadcom BCM440x 
		   PXE (Preboot Execution Environment) Software
				  12/10/2002


b44base.lom: This image consists of the base code (BC) only, for use in
	     a split implementation for LOM applications. 
	     This module should be programmed into the BIOS. 
	     This base-code supports only the PXE software.

b44undi.lom: This image consists of the UNDI code only, for use in
	     a split implementation for LOM applications, where a 
	     BC is present.
	     This module should be programmed into the BIOS.

b44pxe.lom : This is a monolithic image that consists of both the
	     BC and UNDI code. This image is intended for 
	     LOM applications. 


Revision History
================
v 1.0.4 - Added multicast frame support.

v 1.0.3 - Removed 4 second non-bbs support delay. Expecting BBS support.

v 1.0.2 - Added media failure screen message.

v 1.0.1 - Increased performance.

v 1.0.0 - Fixed memory allocation bug.

v 0.0.3 - BETA:Fixed RIS bug & occasional switch compatibility problem.

v 0.0.2 - BETA:Release to fix timeout when copying ghost images.

v 0.0.1 - Engineering Release.

