
Broadcom Corporation 440X Fast Ethernet 10/100 DOS ODI driver.

For use on PCs running DOS version 6.22 only. 

To use to login to a Novell Netware Server use the Novell ZENWorks Starter Pack
to setup and configure your PC.

To login to NETBEUI/NDIS environments please use Novell's ODINSUP.COM protocol
as a link between the B44 DOS ODI driver and the NETBEUI/NDIS protocols.

CUSTOM KEYWORDS in driver v1.10 for net.cfg:

BUSNUM 
DEVNUM
MODEL

The first two keywords are used concurrently and have been included for 
manufacturing purposes.  Do not use them unless you are familiar with PCI
device configuration.
These two keywords are needed if multiple NetXtreme boards are on a system 
and (a) specific NetXtreme adapter/s need to be loaded in specific order.
BUSNUM specifies the PCI bus number and DEVNUM specifies the device
number given to the board when configured by the PCI BIOS.
A PCI device scan utility is needed to find this info.
The values are in decimal.
Example:
	if a PCI scan utility displays card 1 at bus 4 and device 11(hex) and
	card 3 at bus 3 device 13 hex then the following would be put into net.cfg
	to load card 3 first and optionally load card 1 second:


	LINK DRIVER B44
		BUSNUM 3
		DEVNUM 19 (13 hex = 19 decimal)
	LINK DRIVER B44
		BUSNUM 4
		DEVNUM 17 (11 hex = 17 decimal)


The MODEL keyword is for loading the driver only on the first NIC found
that has a sub-vendor ID (SVID) that matches the one set in MODEL. The driver
will ignore all other NICs that do not have a matching SVID.
MODEL expects a decimal number.

Example:
	
	LINK DRIVER B44
		MODEL 5348
