
Broadcom Corporation 10/100/1000 NetXtreme Ethernet DOS ODI driver.

For use on PCs running DOS version 6.22 only. 

To use to login to a Novell Netware Server use the Novell ZENWorks Starter Pack
to setup and configure your PC.

To login to NETBEUI/NDIS environments please use Novell's ODINSUP.COM protocol
as a link between the B57 DOS ODI driver and the NETBEUI/NDIS protocols.

CUSTOM KEYWORDS for net.cfg:

BUSNUM 
DEVNUM
FUNNUM
SUBVID

The first three keywords are used concurrently and have been included for 
manufacturing purposes.  Do not use them unless you are familiar with PCI
device configuration.
These three keywords are needed if multiple NetXtreme boards are on a system 
and (a) specific NetXtreme adapter/s need to be loaded in specific order.
BUSNUM specifies the PCI bus number and DEVNUM specifies the device
number given to the board when configured by the PCI BIOS.

The FUNNUM keyword is used to determine the function/port the driver is to load 
on when using a mutilfunction (multiport) adapter. Function number values are
limited to 0 & 1, for the 1st & 2nd function of the adapter.
The driver will always load on function 0 when this keyword is not used.

The SUBVID keyword is for loading the driver only on the first NIC found
that has a sub-vendor ID (SVID) that matches the one set in NET.CFG. The driver
will ignore all other NICs that do not have a matching SVID.
SUBVID expects a hexadecimal number.

These adapter configuration values are printed out on the screen in hexadecimal
notation when the driver loads.
A PCI device scan utility can also be used to find this information.
The NET.CFG file expects hexadecimal values.

Example:
	If the driver loads on a single adapter, the values displayed on screen
	can be used in the NET.CFG file.
	If a PCI scan utility displays card 1 at bus 4 and device 11(hex) and
	card 3 at bus 3 device 13 hex then the following would be put into net.cfg
	to load card 3 first and optionally load card 1 second:


	LINK DRIVER B57
		BUSNUM 3
		DEVNUM 13 (13 hex = 19 decimal)
	LINK DRIVER B57
		BUSNUM 4
		DEVNUM 11 (11 hex = 17 decimal)

The driver will always load on the first device detected when these keywords are
not used.

Example:
	
	LINK DRIVER B57
		SUBVID 14E4

SUBVID cannot be used with BUSNUM, DEVNUM or FUNNUM.