            SiS 900/7016 PCI Fast Ethernet Adapter Installation
                     for NetWare Server 4.X

[Note]: If you upgraded MSM.NLM, ETHERTSM.NLM and NBI.NLM that was
      created later than Dec 1997, you should use the driver in
      directory \NWSERVER.50.

(1) Modifying an existing NetWare 4.x Server
컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴
    1. Backup NBI.NLM, MSM.NLM and ETHERTSM.NLM to other place.

    2. Please insert SiS 900/7016 driver diskette into floppy disk.

    3. Copy all provided NLM and LAN files into your dos directory
       which include SERVER.EXE.

              COPY A:\NWSERVER.4X\NBI.NLM      C:\NWSERVER
              COPY A:\NWSERVER.4X\MSM.NLM      C:\NWSERVER
              COPY A:\NWSERVER.4X\ETHERTSM.NLM C:\NWSERVER
              COPY A:\NWSERVER.4X\SIS900.LAN  C:\NWSERVER
              COPY A:\NWSERVER.4X\SIS900.LDI  C:\NWSERVER


    4. Start the NetWare Server.

    5. From the Novell Server side, execute "LOAD INSTALL".  Type:

    6. Select <NCF files options>

    7. Select <Edit AUTOEXEC.NCF file>

    8. Add below item into the server's AUTOEXEC.NCF file.

        LOAD C:\NWSERVER\NBI.NLM
        LOAD C:\NWSERVER\MSM.NLM
        LOAD C:\NWSERVER\ETHERTSM.NLM

        LOAD C:\NWSERVER\SIS900 SLOT=1 FRAME=Ethernet_802.3
             NAME=SIS900_1_E83
        BIND IPX SIS900_1_E83 NET=xxxx

        LOAD C:\NWSERVER\SIS900 SLOT=1 FRAME=Ethernet_802.2
             NAME=SIS900_1_E82
        BIND IPX SIS900_1_E82 NET=xxxx

        LOAD C:\NWSERVER\SIS900 SLOT=1 FRAME=Ethernet_II
             NAME=SIS900_1_EII
        BIND IPX SIS900_1_EII NET=xxxx

        LOAD C:\NWSERVER\SIS900 SLOT=1 FRAME=Ethernet_SNAP
             NAME=SIS900_1_ESP
        BIND IPX SIS900_1_ESP NET=xxxx

    9. Restart the server again.

(2) First time installation from the install menu
컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴
    1. Start the NetWare Server.

    2. Execute "LOAD INSTALL" after booting up.  Type,

    3. Select "Driver Options", -> "Configure network drivers", and
       -> "Select a driver".

    4. Press <Insert> key to install an unlisted driver.

    5. Please insert release driver diskette into floppy disk.

    6. Press <F3> to specify a different <PATH>. <PATH> is directory
       which include both SIS900.LAN and SIS900.LDI

          Ex. A:\NETSERVER.4X\

    7. Select "SiS 900/7016 ....".

    8. Specify "SLOT", "FrameSelect", "Node", and "Attachment",
       if necessary.

    9. Select "Save parameters and load driver" after configure
       adapter setting.

    10.NetWare server will loading/binding driver automatically.

(3) The other time installation from the install menu
컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴
    1. Start the NetWare Server.

    2. Execute "LOAD INSTALL" after booting up.  Type,

    3. Select "Driver Options", -> "Configure network drivers", and
       -> "Select a driver".

    4. Select "SiS 900/7016 ...." in Select a driver windows.

    5. Specify "SLOT", "FrameSelect", "Node", and "Attachment",
       if necessary.

    6. Select "Save parameters and load driver" after configure adapter
       setting.

    7. NetWare server will loading/binding driver automatically.


(4) Optional LOAD line parameters
컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴?

    1.SLOT ( Required for multiple cards )

      Specifies the NBI (NetWare Bus Interface) slot number.

      For PCI adapters, SLOT is derived from bus number and device
      location as defined by the PCI specification. One way to determine
      the slot number is to load the driver from the command line. You'll
      be prompted with valid device number(s) for the adapter(s). Select
      one of them.

      Syntax:  SLOT=n     (n = 1,2,3,4,...)


    2.NODE

      Specifies a local administered address (LAA) unique to each adapter.

      Use this option to provide your own unique node address
      for the adapter.  The node address is a 12-digit hexadecimal
      number; the second digit must be one of the following digits: 2, 6,
      A, E.

      Syntax: NODE=xnxxxxxxxxxx

      n = 2, 6, A, E
      x = hexadecimal number

      Default: The adapter's assigned address.

    3.MEDIATYPE

      Specifies the mediatype that is currently used.

      Use this option to force your connection type. We support the
      following media types:

         Type       Ethernet Standard    Duplex
       --------     -----------------    ------
        AUTO          auto-detect         Auto
        UTP           10BASE-T            Half
        UTPFULL       10BASE-T            Full
        FAST          100BASE-T           Half
        FASTFULL      100BASE-T           Full

      Syntax: MEDIATYPE=Type

      Type: see above.

      Default: Auto-Detect.
