IPMI Firmware Release Note
----------------------------
Filename:	SMT_X9_118.bin	ver1.18 Date: 08-16-2011

1. [X9SCD] Adjust fan speed according to the fan mode after post
2. Add mew motherboard X9DRT support

======================================================================================
Filename:	SMT_X9_117.bin	ver1.17 Date: 08-10-2011

1. [X9SCD] Add Fan Control

======================================================================================
Filename:	SMT_X9_116.bin	ver1.16 Date: 08-04-2011

1. [X9SCD] Read CPU Temperature from ME

======================================================================================
Filename:	SMT_X9_115.bin	ver1.15 Date: 07-29-2011

1. [X9DR6] Read CPU Temperature from ME

======================================================================================
Filename:	SMT_X9_114.bin	ver1.14 Date: 07-14-2011

1. Bug fix Event Log description undefined from web GUI(IssusID: 30352, 30327 and 30295)
   Validation: Server Health-> Event Log

2. Bug fix Gateway IP lost
   Validation: change network setting from static to dhcp by using ipmitool or IPMICFG

3. Add iKVM privilege verification
   Validation: virtual media can't be accessed by Operator account

4. [X9DA6] add sensor readings

======================================================================================
Filename:	SMT_X9_113.bin	ver1.13 Date: 06-22-2011

1. Add new motherboard X9DR6 (Support PCHHOT, CPU Error 0/1/2 Event Logs)

2. Bug fix Event Log description undefined from web GUI
   Validation: Server Health-> Event Log

3. Bug fix sensor status icon missing at webpage header
   Validation: summarized sensor status icon located at up-right corner of webpage

4. Bug fix unable to delete newly added Users (IssueID=29907)
5. Bug fix Alert Email description of CPU Overheat event (IssueID=29583)
6. Bug fix SMASH login without password

======================================================================================
Filename:	SMT_X9_112.bin	ver1.12 Date: 06-02-2011

1. Support Circular Buffer evnet logs
   Description: Event logged as FIFO mechanism when number of logs exceeds the maximum fixed-size, 512

2. Support IP Control
   Validation: Verify IP Control feature at IPMI Web-> Configuration-> IP Control

3. [X9SCD] Support Power Monitoring from LM25066 National Chip
   Description: 1. Power Consumption, Input Current & Input Power is monitored at IPMI web-> Miscellaneous-> Power Monitoring
		2. Power consumption is reported to ME through 0xE2 command

======================================================================================
Filename:	SMT_X9_111.bin	ver1.11 Date: 05-26-2011

1. Add "All Event" category as default selection at Event Log page

2. Renew SSL Certificate
Validation:	1) enter Web GUI->Configuration->SSL Certificate, and 2) verify the certificate's validity
*** Note:	Factory Default REQUIRED

3. Change ME slave address to 0x2C in SDR record

======================================================================================
Filename: SMT_X9_110.bin ver1.10 Date: 05-12-2011

1. New feature: launch SOL over SMASH
	Validation: 1) login IPMI SMASH through SSH, 2) follow the command flow: cd system1 -> cd sol1 -> start
	Note: only one SOL session can be launched at a time.

2. Improve security for IPMI Configuration backup
	Validation: Verify the following steps:
		1) open IPMI web 
		2) click on Maintenance -> IPMI Configuration 
		3) save IPMI configuration at local drive, and 
		4) check if the configuration can "NOT" be located at http://ipmi-ip-address/save_config.bin

3. Filter out unknown events #0x17 from ME (IssueID=28839)
	Validation: unknown events #0x17 should be screened out while doing system on/off through IPMI

======================================================================================
Filename:	SMT_X9_109.bin	ver1.09 Date: 04-29-2011

1. Fix CPU overheat false alarm
2. Add new motherboard X9SCD support

======================================================================================
Filename:	SMT_X9_108.bin	ver1.08 Date: 04-01-2011

1. Official release for production

======================================================================================
Filename:	SMT_X9_107.bin	ver1.07 Date: 03-29-2011

1. [X9SCL/M, X9SCA/I] Remove Thermal Trip event log to prevent false alarm

2. Modify default FRU
Description:Board Manufacture modified as "Supermicro" and all other entries cleared
Note:		Required OEM command raw 0x30 0x41(wait for BMC reset) to replace with the new FRU content

======================================================================================
Filename:	SMT_X9_106.bin	ver1.06 Date: 03-18-2011

1. Fix Alert table blank at the webpage when enter more than 29 characters (IssueID: 95761)
   Validation:	1. Connect to IPMI by web browser,
		2. Go to Configuration -> Alerts and select one entry for modify,
		3. In the Message space, enter 30 characters and then save it and then the alert table will be blank.

2. X9SCL/M, X9SCA/I: Support thermal trip event logs

======================================================================================
Filename:	SMT_X9_105.bin	ver1.05 Date: 03-11-2011

1. X9SRI/E: correct sensor readings

======================================================================================
Filename:	SMT_X9_104.bin	ver1.04 Date: 02-23-2011

1. Fix KVM issue with UEFI BIOS
   Validation: reboot system by macro "ctrl+alt+del" and check if key-in is available

2. New feature: Port Configuratioin at Web GUI in Configuration category
   Description: ports of web, web SSL, IKVM server, virtual media are modifiable through web GUI

3. Fix Gateway setting can't work through different subnets 

======================================================================================
Filename:	SMT_X9_103.bin	ver1.03 Date: 02-09-2011

1. Correct size of video/graphics memory as 16MB
*** Note: Requires AC on/off after flashing firmaware

2. Fix cpu temp "Overheat" logged when the reading reports "High"
   Description: CPU temp Overheat should be logged as the reading reaches "Overheat"

3. For security issue, set the privilege of user ID1(Anonymous) with no access and clear jnlp kvm cache
   Validation: 	1. open IPMI web, 2 click Configuration->Users, and 3 check the privilege of user shows Reserved;
		4. launch kvm console, and 5. check if kvm jnlp file is cached after exit

======================================================================================
Filename:	SMT_X9_102.bin	ver1.02 Date: 02-01-2011
1. Add new motherboard support X9SCA/I
2. Add new motherboard support X9SRI/E

======================================================================================
Filename:	SMT_X9SCL_M_V101.bin	ver1.01 Date: 01-11-2010
1. Fix KVM slight flashes of white space while screen resolustion is below 800*640

======================================================================================
Filename:	SMT_X9SCL_M_V100.bin	ver1.00 Date: 12-30-2010
1. change memory configuration for Hynix 800 memory
Note: Please do AC off/on after updating firmware.

======================================================================================
Filename:	SMT_218.bin		ver2.18 Date: 12-17-2010
1. X9SCL/X9SCM: modify Fan5 to FanA

======================================================================================

Filename:	SMT_213.bin		ver2.13	Date: 11-10-2010
1. Add new SSID for X9SCM

======================================================================================

Filename:	SMT_212.bin		ver2.12	Date: 10-25-2010
1. Add new motherboard X9SCL/X9SCM support

