			===========================
			R E L E A S E    N O T E S
			===========================
		   Broadcom Advanced Server Program (BASP)              
			SNMP Instrumentation Agent
			   for Novell NetWare
			     Version 1.03

		   Copyright (c) 2001,2002,2003 Broadcom Corporation
			    All rights reserved.
			       January 13, 2003


Overview
--------
This SNMP agent is designed to support the configuration information 
pertaining to the Broadcom BASP driver for Netware.


Installation
------------
When installed from NWCONFIG or NWINSTALL, the basp.ldi will automatically 
copy the basp.lan, bmapi.nlm & bsnmp.nlm files into the server.

After configuring and running the BASP then binding the BASP to network adapters
load the Broadcom SNMP Instrumentation Agent (BSNMP) with the following steps.

From the Netware Server console command line interface type:

    load bmapi.nlm
    load bsnmp.nlm

SNMP objects
------------
BASP SNMP objects are provided in the BASP-Config.MIB file. 
snmpget and snmpgetnext command can be used to receive the BASP snmp
objects such as:

    snmpget localhost public BASP-Config-MIB::btTeamNumber
    snmpgetnext localhost public BASP-Config-MIB::btTeamNumber

Files
------
    basp.lan
    bmapi.nlm
    bsnmp.nlm
    BASP-CONFIG.MIB
   

Revision History
----------------
01/13/03 - v1.03
	Updated structure support for basp.

03/22/02 - v1.02
	Initial Release.
